MARS In-band Backdoor
General
MARS has an Xbar subsea to allow connection to serial ports on the Cisco’s, EDFA’s and power control.  The Xbar also has one port set for loopback.

Accessing
The Xbar must be set to the appropriate port before serial port access can be done.  The port can be set by either of two ways.  

Method 1 – use webpage to select port
Use a browser to connect to 10.1.128.20/cgi-bin/obc_xbar.

[image: ]

Select the desired port and then connect to 10.1.128.20:7001.

Method 2 – Directly specify port
The port can be directly selected of the desired port number is known.  Simply use a browser to connect to 10.1.128.20/cgi-bin/obc_xbar?port=x
	Where x is one of the following:
1. N/C
2. N/C
3. CiscoA
4. CiscoB
5. East EDFA
6. West EDFA
7. Power Controller
8. Loopback
[bookmark: _GoBack]
image1.png
€ ) @ 10112820/cgi-bin/obc_xbar v & | Q searcn -

Most Visited '} Getig Sarted {3 Handerake Windows ... ] Fee Dev Offers

MARS OBC In-band Backdoor

Select Xbar Port:

1-NC  5-EDE
2-NC  6-EDFAW
3-Ciscod 7-PwiCl

4-CiscoB 8- Loopback

Connect to serial port.
To mamaty conmect, enet 10128120 1001]

Port [] must be between 1 and 8





