BPR-Tilt Deployment on MARS Rev 1
General:
Scheduled deployment date:
June 30, 2010
Scheduled recovery date:
December 14, 2010

Deployment Vessel:

Western Flyer
Recovery Vessel:

Western Flyer

Deployment method:  

Elevator
Special Conditions:



Cable:



70 meter extreme-net with ODI connector on one end

Test Tank Dates:  

MARS Port :
7.
Networking:
Subsurface vlan: 
10.1.17.xxx

Subsurface gateway:
10.1.17.1

MARS O&M reserves address 10.1.17.250 to 10.1.17.255

Only addresses in the range of 10.1.17.2 to 10.1.17. 11 can be mapped to external address

Science vlan:

10.91.47.xxx

Science gateway:
10.91.47.1

MARS O&M reserves address 10.91.47.250 to 10.91.47.255

Only addresses in the range of 10.91.47.2 to 10.91.47. 11 can be mapped to external address

DNS Server #1:
10.91.128.61

DNS Server #2:
10.91.128.62

NTP Server #1:
10.91.128.55

External mapping address range will be 134.89.42.170 to 134.89.42.179.  

A maximum of 10 addresses can be mapped externally.

MARS O&M needs a list of computers by IP address that may access the externally mapped addresses.  (Maximum of 6)

Note:  For WNS testing, the external address range is 134.89.52.170 to 134.89.52.179

Power Requirement:

48 Volts @ 1 amp

Inrush:  10 amp max for 3 ms

