BPR-Tilt Deployment on MARS Rev 4
General:
Scheduled deployment date:
June 30, 2010
Scheduled recovery date:
December 14, 2010

Deployment Vessel:

Western Flyer
Recovery Vessel:

Western Flyer

Deployment method:  

Elevator
Special Conditions:



Cable:



70 meter extreme-net with ODI connector on one end

WNS Testing in Test Tank Dates:  TBD
MARS Port :
7.
Networking:
Subsurface vlan: 
10.1.17.xxx

Subsurface gateway:
10.1.17.1

MARS O&M reserves address 10.1.17.250 to 10.1.17.255

Only addresses in the range of 10.1.17.2 to 10.1.17. 11 can be mapped to external address


Device #1:


Subsea Address:
10.1.17.10



Mapped to:

134.89.42.170   (134.89.52.170 for WNS)


Accessible to:
161.55.192.115



Ports:


Http tcp port 771 and 80






Https 443



Science vlan:

10.91.47.xxx

Science gateway:
10.91.47.1

MARS O&M reserves address 10.91.47.250 to 10.91.47.255

Only addresses in the range of 10.91.47.2 to 10.91.47. 11 can be mapped to external address



No shore side equipment at MBARI planned at this time.
DNS Server #1:
10.91.128.61

DNS Server #2:
10.91.128.62

NTP Server #1:
10.91.128.55

External mapping address range will be 134.89.42.170 to 134.89.42.179.  

A maximum of 10 addresses can be mapped externally.

MARS O&M needs a list of computers by IP address that may access the externally mapped addresses.  (Maximum of 6)

Note:  For WNS testing, the external address range is 134.89.52.170 to 134.89.52.179

Power Requirement:

48 Volts expected draw is 200 ma continuous.

May have additional 1.5 amps draw for 6 hours after turn on for heater.

Inrush:  Limit is 10 amp max for 3 ms.  Reported as 2 amps for 5 ms
