Note:  Changed items are in red
GSSM Deployment on MARS Rev 3
General:
Scheduled deployment date:
June 13, 2017 
Scheduled recovery date:
~June 2018
Deployment Vessel:

Rachael Carson
Recovery Vessel:

Rachael Carson
Deployment method:  


Special Conditions:  
Cable:  50 meter with SIIM can and 10 meter ODI oil filled hose. 

Test Tank Dates:  May 24 & 25 2017
MARS Port:
2
Networking:
Subsurface vlan: 
10.1.12.xxx

Subsurface gateway:
10.1.12.1

MARS O&M reserves address 10.1.12.250 to 10.1.12.255

Only addresses in the range of 10.1.12.2 to 10.1.12.11 can be mapped externally
Device

WNS External
MARS External
MARS Subnet

------

------------
-------------
-----------

GSSM


134.89.52.122
134.89.42.122
10.1.12.2

Science vlan:

10.91.42.xxx

Science gateway:
10.91.42.1

MARS O&M reserves address 10.91.42.250 to 10.91.42.255

Only addresses in the range of 10.91.42.2 to 10.91.42.11 can be mapped to externally
Device

WNS External
MARS External
MARS Subnet

------

------------
-------------
-----------
GSSM Computer
134.89.52.123
134.89.42.123
10.91.42.3

Protocols: TCP/IP, HTTP, FTP, SSH, VPN, Remote Desktop

External mapping address range will be 134.89.42.120 to 134.89.42.129.  

A maximum of 10 addresses can be mapped externally.

UW/APL external address to have access:
128.208.79.248

128.208.79.39

Note:  For WNS testing, the external address range is 134.89.52.120 to 134.89.52.129

Power Requirement:

375 volts @ 30 watts
DNS Server #1:
10.91.128.61

DNS Server #2:
10.91.128.62

NTP Server #1:
10.91.128.55

