Looking Deployment on MARS Rev 1
General:
Scheduled deployment date:
March 9, 2010
Scheduled recovery date:
September 30, 2010

Deployment Vessel:

Western Flyer
Recovery Vessel:

Western Flyer

Deployment method:  

Unknown

Special Conditions:  
Cable:  70 meter extreme-net with ODI connector on one end

Test Tank Dates:  

MARS Port:
1.
Networking:
Subsurface vlan: 
10.1.15.xxx

Subsurface gateway:
10.1.15.1

MARS O&M reserves address 10.1.15.250 to 10.1.15.255

Only addresses in the range of 10.1.15.2 to 10.1.15. 11 can be mapped to externally
Science vlan:

10.91.45.xxx

Science gateway:
10.91.45.1

MARS O&M reserves address 10.91.45.250 to 10.91.45.255

Only addresses in the range of 10.91.45.2 to 10.91.45.11 can be mapped to externally
DNS Server #1:
10.91.128.61

DNS Server #2:
10.91.128.62

NTP Server #1:
10.91.128.55

External mapping address range will be 134.89.42.150 to 134.89.42.159.  

A maximum of 10 addresses can be mapped externally.

MARS O&M needs a list of computers by IP address that may access the externally mapped addresses.  (Maximum of 6)

Note:  For WNS testing, the external address range is 134.89.52.150 to 134.89.52.159

Power Requirement:

