Looking Deployment on MARS Rev 3
General:
Scheduled deployment date:
March 26, 2010 (Not confirmed)
Scheduled recovery date:
September 30, 2010

Deployment Vessel:

Point Lobos
Recovery Vessel:

Western Flyer

Deployment method:  

Elevator
Special Conditions:  
Cable:  70 meter extreme-net with ODI connector on one end.  Deploy with spool.
Test Tank Dates:  March 15, 2010 through March 17, 2010
MARS Port:
1.
Networking:
Subsurface vlan: 
10.1.15.xxx

Subsurface gateway:
10.1.15.1

MARS O&M reserves address 10.1.15.250 to 10.1.15.255

Only addresses in the range of 10.1.15.2 to 10.1.15. 11 can be mapped to externally
Device #1:



Subsea address:
10.1.15.10 

Mapped to: 

134.89.42.150
UDP Ports:

5330-5339

Accessible to:
132.239.4.0/24

Device #2: 
Subsea address:
10.1.15.11 

Mapped to: 

134.89.42.151

TCP port:

6510 (data) and 22 (ssh)

Accessible to:
132.239.4.0/24

Science vlan:

10.91.45.xxx

Science gateway:
10.91.45.1

MARS O&M reserves address 10.91.45.250 to 10.91.45.255

Only addresses in the range of 10.91.45.2 to 10.91.45.11 can be mapped to externally
No shore side equipment at MBARI planned at the present time.
DNS Server #1:
10.91.128.61

DNS Server #2:
10.91.128.62

NTP Server #1:
10.91.128.55

External mapping address range will be 134.89.42.150 to 134.89.42.159.  

A maximum of 10 addresses can be mapped externally.

MARS O&M needs a list of computers by IP address that may access the externally mapped addresses.  (Maximum of 6)

Note:  For WNS testing, the external address range is 134.89.52.150 to 134.89.52.159

Power Requirement:

48 volts @ 5 watts
No 375 volts

