PHOBOS Instrument Information
Main Controller				10.1.14.2	134.89.42.142
DigiServer for camera control		10.1.14.3	134.89.42.143
DigiServer for CTD and ADCP		10.1.14.4	134.89.42.144
HD Video Feed				10.1.14.6	134.89.42.146
Light Control				10.1.14.8	134.89.42.148
Surface Computer				10.91.44.5	134.89.42.145

The four science instruments are connected to the DigiServer.
Instrument 	Port	Baud	Control computer mapping	SSDS ID
ADCP		1	9600		COM6				1764
Fluor		2	19.2K		COM7				1535
CTD		3	9600		COM8				1806
O2		4	9600		COM9				1804
Camera		38.4K		COM12
Pan & Tilt		9600		COM13
Note:  Com5 use to be MINK10L
Perle Server		DigiServer		HD Video Feed
       admin		     root			     admin
      supervisor		     dbps			     admin
Control Computer		HD Decoder
	dmolab			     admin
	mbarilab		     admin


Location	Pan		Tilt
Comp		15		230
White card	37		174
Bones		71.7		155.5

