PhoBOS Video
There is a high definition camera on PhoBOS.  The video stream from the camera is encoded by a Teradek Cube.  The cube’s IP address is 10.1.14.6.  The cube pushes the video to Marvin, IP address 134.89.12.79 on port 9710.  It is a udp stream.  Marvin does a multicast of the video to 234.134.89.2 on port 1234, also udp.  Marvin uses VLC to receive and transmit the video.
