Phobos Deployment on MARS – Rev 2
General:
Scheduled deployment date:  June ??, 2010

Vessel:
  Pt Lobos/Ventana
Deployment method:  Front Porch
Special Conditions:  Will sit on top of MARS
Cable:  2 meter oil filled hose with ODI connector on one end

Test Tank Dates:  June ??, 2010
Phobos will be connected to port 4 on MARS.
Networking:
Subsurface vlan: 
10.1.14.xxx

Subsurface gateway:
10.1.14.1

MARS O&M reserves address 10.1.14.250 to 10.1.14.255

Only addresses in the range of 10.1.14.2 to 10.1.14.11 can be mapped to external address

Three subsea addresses required.  All required to be mapped to 134 addresses accessed from within the MBARI network.


DigiServer for CTD and ADCP
10.1.14.2
134.89.42.142


DigiServer for camera control
10.1.14.3
134.89.42.143


Video server for camera

10.1.14.4
134.89.42.144

Science vlan:

10.91.44.xxx

Science gateway:
10.91.44.1

MARS O&M reserves address 10.91.44.250 to 10.91.44.255

Only addresses in the range of 10.91.44.2 to 10.91.44.11 can be mapped to external address

No shore side systems within MARS network.

DNS Server #1:
10.91.128.61

DNS Server #2:
10.91.128.62

NTP Server #1:
10.91.128.55

External mapping address range will be 134.89.42.140 to 134.89.42.149.  

A maximum of 10 addresses can be mapped externally.

MARS O&M needs a list of computers by IP address that may access the externally mapped addresses.  (Maximum of 6)

Note:  For WNS testing, the external address range is 134.89.52.140 to 134.89.52.149

Power Requirement:

48 volts - none
375 volts – 1 amp max
Inrush current – 15 amps maximum, 3 ms duration.
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