Phobos Deployment on MARS – Rev 10
Changes in red
General:
Test Tank Dates:  Week of July 15, 2013
Scheduled deployment date:  July 25, 2013
Vessel:	  Rachel Carson
Deployment method:  Float pack
Weight in air:  420 lbs
Weight In water:  185 lbs
Cable:  70 meter to SIIM to 5 meter oil filled hose with ODI connector (90 degree pen)
Port:  4

Networking:
Subsurface vlan: 	10.1.14.xxx
Subsurface gateway:	10.1.14.1
MARS O&M reserves address 10.1.14.250 to 10.1.14.255
Only addresses in the range of 10.1.14.2 to 10.1.14.11 can be mapped to external address

Four subsea addresses required (10.1.14.6 added since last deployment)
Main Controller			10.1.14.2	134.89.42.142
Perle Server for camera control	10.1.14.3	134.89.42.143
	DigiServer for CTD and ADCP	10.1.14.4	134.89.42.144
	HD Video Feed			10.1.14.6	134.89.42.146
	
Science vlan:		10.91.44.xxx
Science gateway:	10.91.44.1
MARS O&M reserves address 10.91.44.250 to 10.91.44.255
Only addresses in the range of 10.91.44.2 to 10.91.44.11 can be mapped to external address

Two surface addresses required.
Control computer			10.91.44.5	134.89.42.145
HD Decode				10.91.44.7	134.89.42.147

DNS Server #1:	10.91.128.61
DNS Server #2:	10.91.128.62
NTP Server #1:	10.91.128.55

External mapping address range will be 134.89.42.140 to 134.89.42.149.  
A maximum of 10 addresses can be mapped externally.
MARS O&M needs a list of computers by IP address that may access the externally mapped addresses.  (Maximum of 6)
Note:  For WNS testing, the external address range is 134.89.52.140 to 134.89.52.149




Power Requirement:
48 volts - none

375 volts – 1 amp max
Inrush current – 15 amps maximum, 3 ms duration.


