Tongji Deployment on MARS Rev 1
General:
Scheduled deployment date:
TBD 
Scheduled recovery date:
TBD
Deployment Vessel:

TBD
Recovery Vessel:

TBD
Deployment method:  

TBD
Special Conditions:  

Cable:  

Test Tank Dates:  

MARS Port:
6.
Power Requirement:

48 volts – Not used
375 volts - TBD
Networking:
DNS Server #1:
10.91.128.61

DNS Server #2:
10.91.128.62

NTP Server #1:
10.91.128.55

Netmask

255.255.255.0

Subsurface vlan: 
10.1.16.xxx

Subsurface gateway:
10.1.16.1

MARS O&M reserves address 10.1.16.250 to 10.1.16.255

Five subsea network devices


Subsea #1

10.1.16.7


Subsea #2

10.1.16.8


Subsea #3

10.1.16.9


Subsea #4

10.1.16.10


Subsea #5

10.1.16.11

Science vlan:

10.91.46.xxx

Science gateway:
10.91.46.1

MARS O&M reserves address 10.91.46.250 to 10.91.46.255

Five science vlan computers

WEB Server

10.91.46.2

134.89.42.162


Data Server

10.91.46.3


Desktop #1

10.91.46.4


Desktop #2

10.91.46.5


Laptop

10.91.46.6

Currently, only the WEB Server will be mapped to an external address.  
MARS Operations needs the IP address of systems (limit of 6) that are to have access this address.  

Ports that will be opened for connection to the WEB Server will be TCP ports 8000 and 8200 and HTTP port 80.
Note:  For WNS testing, the external address will be 134.89.52.162
