(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 1.6)
    (drawings 21)
    (tracks 131)
    (zones 0)
    (modules 51)
    (nets 27)
  )
  (page B)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.625)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 63.5 215.9)
    (visible_elements FFFDFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /+375V)
  (net 2 /+9V)
  (net 3 "Net-(0.0048_Plus1-Pad1)")
  (net 4 /48V_RTN)
  (net 5 "Net-(0.0375_Plus1-Pad1)")
  (net 6 /375V_RTN)
  (net 7 "Net-(375_LED1-Pad1)")
  (net 8 "Net-(375_TP1-Pad1)")
  (net 9 "Net-(48_LED1-Pad1)")
  (net 10 /+48V)
  (net 11 /9V_RTN)
  (net 12 "Net-(F1-Pad2)")
  (net 13 "Net-(R1-Pad2)")
  (net 14 "Net-(R2-Pad2)")
  (net 15 "Net-(R3-Pad2)")
  (net 16 "Net-(R7-Pad2)")
  (net 17 "Net-(R8-Pad2)")
  (net 18 "Net-(R10-Pad1)")
  (net 19 "Net-(R10-Pad2)")
  (net 20 "Net-(R11-Pad2)")
  (net 21 "Net-(R12-Pad2)")
  (net 22 "Net-(R13-Pad2)")
  (net 23 "Net-(R14-Pad2)")
  (net 24 "Net-(R15-Pad2)")
  (net 25 "Net-(R17-Pad2)")
  (net 26 "Net-(R20-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+375V)
    (add_net /+48V)
    (add_net /+9V)
    (add_net /375V_RTN)
    (add_net /48V_RTN)
    (add_net /9V_RTN)
    (add_net "Net-(0.0048_Plus1-Pad1)")
    (add_net "Net-(0.0375_Plus1-Pad1)")
    (add_net "Net-(375_LED1-Pad1)")
    (add_net "Net-(375_TP1-Pad1)")
    (add_net "Net-(48_LED1-Pad1)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R20-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
  )
  (module Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork (layer F.Cu) (tedit 5C89BF14)
    (at 142.24 107.95)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference +375V1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 /+375V))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork (layer F.Cu) (tedit 5C89BF14)
    (at 138.43 208.28)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference +9V1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 /+9V))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork (layer F.Cu) (tedit 5C89BF14)
    (at 120.65 208.28)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference 0.0048_Plus1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 "Net-(0.0048_Plus1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork (layer F.Cu) (tedit 5C89BF14)
    (at 128.27 208.28)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference 0.0048_Rtn1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 /48V_RTN))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork (layer F.Cu) (tedit 5C89BF14)
    (at 195.58 208.28)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference 0.0375_Plus1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 5 "Net-(0.0375_Plus1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork (layer F.Cu) (tedit 5C89BF14)
    (at 203.2 208.28)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference 0.0375_Rtn1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 6 /375V_RTN))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork (layer F.Cu) (tedit 5C89BF14)
    (at 161.29 208.28)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference 375_LED1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 7 "Net-(375_LED1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork (layer F.Cu) (tedit 5C89BF14)
    (at 167.64 208.28)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference 375_LED_Rtn1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 6 /375V_RTN))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork (layer F.Cu) (tedit 5C89BF14)
    (at 184.15 208.28)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference 375_Rtn_TP1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 6 /375V_RTN))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork (layer F.Cu) (tedit 5C89BF14)
    (at 177.8 208.28)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference 375_TP1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 8 "Net-(375_TP1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork (layer F.Cu) (tedit 5C89BF14)
    (at 156.21 107.95)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference 375V_RTN1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 6 /375V_RTN))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork (layer F.Cu) (tedit 5C89BF14)
    (at 87.63 208.28)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference 48_LED1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 9 "Net-(48_LED1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork (layer F.Cu) (tedit 5C89BF14)
    (at 95.25 208.28)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference 48_LED_Rtn1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 /48V_RTN))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork (layer F.Cu) (tedit 5C89BF14)
    (at 88.9 107.95)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference 48_Plus1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 10 /+48V))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork (layer F.Cu) (tedit 5C89BF14)
    (at 104.14 208.28)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference 48_Plus_TP1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 10 /+48V))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork (layer F.Cu) (tedit 5C89BF14)
    (at 101.6 107.95)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference 48_Rtn1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 /48V_RTN))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork (layer F.Cu) (tedit 5C89BF14)
    (at 111.76 208.28)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference 48_Rtn_TP1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 /48V_RTN))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork (layer F.Cu) (tedit 5C89BF14)
    (at 146.05 208.28)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference 9V_RTN1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 11 /9V_RTN))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-201_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 87.63 130.81 270)
    (descr "Diode, DO-201 series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.53*5.21mm^2, , http://www.diodes.com/_files/packages/DO-201.pdf")
    (tags "Diode DO-201 series Axial Horizontal pin pitch 15.24mm  length 9.53mm diameter 5.21mm")
    (fp_text reference D1 (at 7.62 -3.725 90) (layer F.SilkS))
    (fp_text value 1N5369B (at 7.62 3.725 90) (layer F.Fab))
    (fp_text user %R (at 8.33475 0 90) (layer F.Fab))
    (fp_text user K (at 0 -2.3 90) (layer F.Fab))
    (fp_text user K (at 0 -2.3 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 10 /+48V))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 /48V_RTN))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-201_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-201_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 190.5 177.8)
    (descr "Diode, DO-201 series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.53*5.21mm^2, , http://www.diodes.com/_files/packages/DO-201.pdf")
    (tags "Diode DO-201 series Axial Horizontal pin pitch 15.24mm  length 9.53mm diameter 5.21mm")
    (fp_text reference D2 (at 0 -3.81) (layer F.SilkS))
    (fp_text value 1N5369B (at 7.62 3.725) (layer F.Fab))
    (fp_text user K (at 0 -2.3) (layer F.SilkS))
    (fp_text user K (at 0 -2.3) (layer F.Fab))
    (fp_text user %R (at 8.33475 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 /375V_RTN))
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "Net-(0.0375_Plus1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-201_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 88.9 123.19)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference F1 (at 7.62 -3.37) (layer F.SilkS))
    (fp_text value Fuse_Small (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(F1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 /+48V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_4.3mm_M4 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 76.2 114.3)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr virtual)
    (fp_text reference H1 (at 0 -5.3) (layer F.SilkS))
    (fp_text value MountingHole (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 2.54 -5.08) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_4.3mm_M4 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 215.9 114.3)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr virtual)
    (fp_text reference H2 (at 0 -5.3) (layer F.SilkS))
    (fp_text value MountingHole (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 2.54 -5.08) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_4.3mm_M4 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 76.2 203.2)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr virtual)
    (fp_text reference H3 (at 0 -5.3) (layer F.SilkS))
    (fp_text value MountingHole (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_4.3mm_M4 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 215.9 203.2)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr virtual)
    (fp_text reference H4 (at 0 -5.3) (layer F.SilkS))
    (fp_text value MountingHole (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 85.09 157.48)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R1 (at -2.54 -1.27) (layer F.SilkS))
    (fp_text value 1.21k (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 /+48V))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 85.09 163.83)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R2 (at -2.54 -1.27) (layer F.SilkS))
    (fp_text value 1.21k (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "Net-(R2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 85.09 176.53)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R4 (at -2.54 -1.27) (layer F.SilkS))
    (fp_text value 1.21k (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(48_LED1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 107.95 156.21 270)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R5 (at 0 -3.81 180) (layer F.SilkS))
    (fp_text value 100k (at 7.62 3.37 90) (layer F.Fab))
    (fp_text user %R (at 7.62 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 /+48V))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(0.0048_Plus1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 107.95 177.8 270)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R6 (at 0 -3.81 180) (layer F.SilkS))
    (fp_text value "10 Ohms" (at 7.62 3.37 90) (layer F.Fab))
    (fp_text user %R (at 7.62 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 /48V_RTN))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(0.0048_Plus1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 142.24 121.92)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R7 (at -3.81 -0.83) (layer F.SilkS))
    (fp_text value 3.83k (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 "Net-(R7-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 /+375V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 142.24 129.54)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R8 (at -3.81 -0.83) (layer F.SilkS))
    (fp_text value 3.83k (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 "Net-(R7-Pad2)"))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 142.24 137.16)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R9 (at -3.81 -0.83) (layer F.SilkS))
    (fp_text value 3.83k (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 "Net-(R10-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 142.24 144.78)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R10 (at -3.81 -0.83) (layer F.SilkS))
    (fp_text value 3.83k (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 "Net-(R10-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 19 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 142.24 152.4)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R11 (at -3.81 -0.83) (layer F.SilkS))
    (fp_text value 3.83k (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 20 "Net-(R11-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 19 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 142.24 160.02)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R12 (at -3.81 -0.83) (layer F.SilkS))
    (fp_text value 3.83k (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 20 "Net-(R11-Pad2)"))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 21 "Net-(R12-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 142.24 167.64)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R13 (at -3.81 -0.83) (layer F.SilkS))
    (fp_text value 3.83k (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 22 "Net-(R13-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 21 "Net-(R12-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 142.24 175.26)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R14 (at -3.81 -0.83) (layer F.SilkS))
    (fp_text value 3.83k (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 22 "Net-(R13-Pad2)"))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 "Net-(R14-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 142.24 182.88)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R15 (at -3.81 -0.83) (layer F.SilkS))
    (fp_text value 3.83k (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 24 "Net-(R15-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 "Net-(R14-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 142.24 190.5)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R16 (at -3.81 -1.27) (layer F.SilkS))
    (fp_text value 3.83k (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 24 "Net-(R15-Pad2)"))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(375_LED1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 166.37 144.78)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R17 (at -3.81 -1.27) (layer F.SilkS))
    (fp_text value 261k (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 /+375V))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 25 "Net-(R17-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 166.37 152.4)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R18 (at -3.81 -1.27) (layer F.SilkS))
    (fp_text value 261k (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(375_TP1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 25 "Net-(R17-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 166.37 160.02)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R19 (at -3.81 -1.27) (layer F.SilkS))
    (fp_text value 90.9k (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(375_TP1-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 /375V_RTN))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 191.77 144.78)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R20 (at -3.81 -1.27) (layer F.SilkS))
    (fp_text value 261k (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 26 "Net-(R20-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 /+375V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 191.77 152.4)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R21 (at -3.81 -1.27) (layer F.SilkS))
    (fp_text value 261k (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 26 "Net-(R20-Pad2)"))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(0.0375_Plus1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 191.77 160.02)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R22 (at -3.81 -1.27) (layer F.SilkS))
    (fp_text value "90.9 Ohms" (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(0.0375_Plus1-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 /375V_RTN))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3266W_Vertical (layer F.Cu) (tedit 5A3D4994)
    (at 196.85 170.18 180)
    (descr "Potentiometer, vertical, Bourns 3266W, https://www.bourns.com/docs/Product-Datasheets/3266.pdf")
    (tags "Potentiometer vertical Bourns 3266W")
    (fp_text reference RV1 (at 3.81 2.54) (layer F.SilkS))
    (fp_text value "500 Ohms" (at -2.54 4.73) (layer F.SilkS))
    (fp_text user %R (at -3.175 1.23) (layer F.Fab) hide)
    (pad 3 thru_hole circle (at -5.08 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /375V_RTN))
    (pad 2 thru_hole circle (at -2.54 2.54 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /375V_RTN))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(0.0375_Plus1-Pad1)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3266W_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3266W_Vertical (layer F.Cu) (tedit 5A3D4994)
    (at 171.45 170.18 180)
    (descr "Potentiometer, vertical, Bourns 3266W, https://www.bourns.com/docs/Product-Datasheets/3266.pdf")
    (tags "Potentiometer vertical Bourns 3266W")
    (fp_text reference RV2 (at 3.81 2.54) (layer F.SilkS))
    (fp_text value 200k (at -2.54 4.73) (layer F.Fab))
    (fp_text user %R (at -3.175 1.23) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(375_TP1-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 2.54 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /375V_RTN))
    (pad 3 thru_hole circle (at -5.08 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /375V_RTN))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3266W_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:SUS01 (layer F.Cu) (tedit 5D214FA7)
    (at 99.06 130.81)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U1 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value SUS01 (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(F1-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /48V_RTN))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /+9V))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /9V_RTN))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /9V_RTN))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /+9V))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /48V_RTN))
    (pad 16 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(F1-Pad2)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-201_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 166.37 177.8)
    (descr "Diode, DO-201 series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.53*5.21mm^2, , http://www.diodes.com/_files/packages/DO-201.pdf")
    (tags "Diode DO-201 series Axial Horizontal pin pitch 15.24mm  length 9.53mm diameter 5.21mm")
    (fp_text reference D3 (at 1.27 -3.725) (layer F.SilkS))
    (fp_text value 1N5369B (at 7.62 3.725) (layer F.Fab))
    (fp_text user %R (at 8.33475 0) (layer F.Fab))
    (fp_text user K (at 0 -2.3) (layer F.Fab))
    (fp_text user K (at 0 -2.3) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "Net-(375_TP1-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 /375V_RTN))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-201_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 85.09 170.18)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R3 (at -2.54 -1.27) (layer F.SilkS))
    (fp_text value 1.21k (at 7.62 3.37) (layer F.Fab))
    (fp_text user %R (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "Net-(R2-Pad2)"))
    (pad 2 thru_hole oval (at 15.24 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "375 VOLTS" (at 147.32 116.84) (layer F.SilkS))
  (gr_text "48 VOLTS" (at 111.76 127) (layer F.SilkS))
  (gr_text "48 VOLTS" (at 83.82 127) (layer F.SilkS))
  (gr_text "BOT SILK" (at 215.9 190.5) (layer B.SilkS))
  (gr_text "TOP SILK" (at 215.9 182.88) (layer F.SilkS))
  (gr_text "TOP CU" (at 215.9 185.42) (layer F.Cu))
  (gr_text "BOT CU" (at 215.9 187.96) (layer B.Cu))
  (gr_text "DWG: 100221340\nCopyright (c) MBRI 2019" (at 209.55 133.35) (layer B.SilkS))
  (gr_text "MARS WET NODE SIMULATOR\nVOLTAGE TEST BOX\nREV A  KICAD" (at 210.82 127) (layer B.SilkS))
  (gr_text "375 VOLTS" (at 196.85 140.97) (layer F.SilkS))
  (gr_text "375 VOLTS" (at 171.45 140.97) (layer F.SilkS))
  (gr_text "DANGER\nHAZARDOUS\nVOLTAGE" (at 125.73 119.38) (layer B.SilkS))
  (gr_text "DANGER\nHAZARDOUS\nVOLTAGE" (at 125.73 109.22) (layer F.SilkS))
  (gr_text "DWG: 100221340\nCopyright (c) MBARI 2019" (at 182.88 130.81) (layer F.SilkS))
  (gr_text KiCAD (at 193.04 118.11) (layer F.SilkS))
  (gr_text "REV A  " (at 177.8 118.11) (layer F.SilkS))
  (gr_text "MARS WET NODE SIMULATOR\nVOLTAGE TEST BOX" (at 186.69 113.03) (layer F.SilkS))
  (gr_line (start 63.5 101.6) (end 63.5 215.9) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 228.6 101.6) (end 63.5 101.6) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 228.6 215.9) (end 228.6 101.6) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.5 215.9) (end 228.6 215.9) (layer Edge.Cuts) (width 0.1))
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch none 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.291127 127) (xy 173.431127 127) (xy 173.431127 120.65) (xy 196.291127 120.65)
      )
    )
  )
)
