Standard, Straight-Through Wiring Diagram(both ends are the same):

	RJ45 Pin #
	Wire Color
(T568A)
	Wire Diagram
(T568A)
	10Base-T Signal
100Base-TX Signal
	1000Base-T Signal

	1
	White/Green
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	Transmit+
	BI_DA+

	2
	Green
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	Transmit-
	BI_DA-

	3
	White/Orange
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	Receive+
	BI_DB+

	4
	Blue
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	Unused
	BI_DC+

	5
	White/Blue
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	Unused
	BI_DC-

	6
	Orange
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	Receive-
	BI_DB-

	7
	White/Brown
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	Unused
	BI_DD+

	8
	Brown
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	Unused
	BI_DD-


Straight-Through Ethernet Cable Pin Out for T568A 

	RJ45 Pin #
	Wire Color
(T568B)
	Wire Diagram
(T568B)
	10Base-T Signal
100Base-TX Signal
	1000Base-T Signal

	1
	White/Orange
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	Transmit+
	BI_DA+

	2
	Orange
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	Transmit-
	BI_DA-

	3
	White/Green
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	Receive+
	BI_DB+

	4
	Blue
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	Unused
	BI_DC+

	5
	White/Blue
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	Unused
	BI_DC-

	6
	Green
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	Receive-
	BI_DB-

	7
	White/Brown
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	Unused
	BI_DD+

	8
	Brown
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	Unused
	BI_DD-


Straight-Through Ethernet Cable Pin Out for T568B 

Crossover Cable Wiring Diagram(T568B):

	RJ45 Pin # (END 1)
	Wire Color
	Diagram End #1
	RJ45 Pin # (END 2)
	Wire Color
	Diagram End #2

	1
	White/Orange
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	1
	White/Green
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	2
	Orange
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	2
	Green
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	3
	White/Green
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	3
	White/Orange
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	4
	Blue
	[image: image23.png]



	4
	White/Brown
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	5
	White/Blue
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	5
	Brown
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	6
	Green
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	6
	Orange
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	7
	White/Brown
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	7
	Blue
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	8
	Brown
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	8
	White/Blue
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Crossover Ethernet Cable Pin Outs 

+Note: The crossover ethernet cable layout is suitable for 1000Base-T operation, all 4 pairs are crossed. 
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Female
	Male
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