Cable Monitoring Plan – Notes
Propose 2 survey regions with a control and cable area in each.

1. Survey next to node
Control area ~300m away

2. Survey area on neck of Smooth Ridge where cable not buried
Control area ~300m away

Conduct 2-hour video survey of each of the four areas (2 full dive days).

Cover approx. 1km of cable length.

