General Best Management Practices for upland and in-water work.

· Locate the entry pit and exit pit at a sufficient elevation to avoid inundation by tidal activity.
· Contain the spoils stored from the excavation of the entry/exit pits using silt fencing, to avoid sediment transport.

· If drilling mud does not congeal, erect isolation/containment environments (underwater booms and/or turbidity curtains);

· If the frac-out becomes excessively large, call in a spill response team to contain and clean up excess drilling mud in the water.

· Undertake and complete proper disposal of excess spoils; backfilling and restoring the original contour to the entry/exit pits.

· If a frac-out occurs, a qualified biological monitor should monitor the clean up of the drilling mud.

If a frac-out is identified in an upland area the following will be implemented:

· All work stops, including the recycling of drilling mud/lubricant to reduce pressure and keep excess mud from escaping through the identified fracture.

· Isolate the frac-out in upland areas with hay bales, sand bags, or silt fencing to surround and contain the drilling mud.

· Report all bentonite seeps into waters of the State or sensitive habitat immediately to the Project's resource coordinator, and the appropriate resource agencies.

· Consult with required regulatory agencies regarding next appropriate action regarding the clean up of the drilling mud.

· Once clean up has been completed the area will be restored to preconstruction conditions in consultation with regulatory agencies.

If a frac-out occurs within the waters of the State the following will be implemented:

· All work stops, including the recycling of drilling mud/lubricant to reduce pressure and keep excess mud from escaping through the identified fracture.

· After the frac-out has occurred the site would be monitored to determine if
the drilling mud congeals to determine the appropriate clean-up response.

· Consult with regulatory agencies to determine the next appropriate step to
clean-up the frac-out.
