ENVIRONMENTAL CROSSINGS, INC.

RIG NO. 3

AMERICAN AUGERS DD-220 (1995)
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American Auger DD-220

AMERICAN AUGERS DD-220:




RATED TO 215K PUSH AND PULL




RATED TO 30K TWO SPEED ROTARY TORQUE




3406 TURBO CAT POWERED 440 HP




CONTROLS SAVER SUNSTRAND JOYSTICKS




OPEN BREAK OUT TRAVEL VISES




ROTARY BRAKES




HYDRAULIC OIL HEAT EXCHANGER




TRAILER LOW BOY (45 FT) NON PERMIT LOAD




TRIPLE CYLINDER WRENCH CLAMP

ECI MUD SYSTEM:

ECI DESIGN AND BUILT
     

200 BBL CAPACITY

3408 CAT POWERED

ALLISION TRANSMISSION (5 SPEED)

DE-SANDERS (1000 GPM)

TRAILER MOUNTED (52 FT) NON 

PERMIT LOAD

DE-SILTERS (1000 GPM)

5 4” X 5” (50 HP) CHARGE AND MIXING PUMPS

ELLIS WILLIAMS 446 MUD PUMP (CAPACITY 450 GPM)

4 LINEAR TWO PANEL SHAKERS

150 GALLON FUEL CAPACITY
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Mud System

CONTROL UNIT:
WELLS CARGO 22 FT. X 8 FT. OFFICE UNIT




MOUNTED SAVER SUNSTRAND DRILLER CONTROLS




STEER OPERATORS EQUIPMENT

TOOL VAN:

FREIGHT TRAILER (45 FT)




AIR COMPRESSOR




MECHANICS SHOP




PARTS HOUSE




3406 CAT POWERED GEN 260 KW

MISCELLANEOUS EQUIPMENT:



2-30 FT MONEL DRILL COLLARS




JETTING ASSEMBLIES




ASSORTED FLY CUTTERS (REAMERS)




ASSORTED BARREL REAMERS




4000 FT S-135 (19.5 LB PER FT) DRILL PIPE



PIPE TRAILERS




4 IN HYD SUB PUMPS




FLAT MUD HOSE (1500 FT) AND CAM LOCK FITTINGS




EXTRA HYD HOSES AND FITTINGS




EXTRA HYD PUMPS AND FITTINGS




EXTRA HYD MOTORS AND FITTINGS




SUBS




PIPE TONGS




HAND TOOLS




MISC SPARE PARTS:  PUMP, HYD 





(ESTIMATED $30K SPARES)

ALL ENVIRONMENTAL CROSSINGS’ EQUIPMENT IS MAINTAINED IN EXCELLENT OPERATION AND COSMETIC CONDITION.
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