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MARS Cable Route Application 
Revision of Shore Landing Information

September 8, 2004


In the original application packet, we described the onshore facilities for the MARS project in Section E2. We have recently been informed that the Duke Energy landing, originally described as the “Northern Shore Landing Alternative,” is no longer an option due to a policy change within Duke Energy. MBARI still has permission from Duke Energy to use the existing fuel oil pipeline to bring the cable onshore. However, we can no longer place a shore facility on their property. Therefore, MBARI is submitting the following information to replace the original Section E2.

E2. Onshore Facilities

Shore Landings

There are three possible shore landing options for the MARS cable—two options utilizing the Duke Energy fuel oil pipeline in the north harbor entrance, and one option using the planned Moss Landing Marine Laboratories pier south of the canyon head. Figure 1 is an aerial view of the Moss Landing region showing the relative location of these sites.

Option 1 – Duke Energy Pipeline to MBARI Building D

Option 1 involves pulling the cable through the existing Duke Energy pipeline. The pipeline extends in a west-northwest direction from the shore to a water depth of roughly 18 meters (see Figure E-1 in the original application). The position of the end of the pipeline is 36(48.719' N, –121(48.037' W and is located approximately 153 meters from shore. The pipe is 18"–24" carbon steel and has been well maintained by Duke Energy. MBARI will attempt to modify the cap at the ocean end of the pipeline to include a seal allowing the MARS cable to enter the pipeline and remain sealed for corrosion protection. Duke Energy has reviewed their records and do not believe the pipeline is currently under lease with the State Lands Commission. Please see Figures E-2, E-3, and E-4 in the original application binder for further details of the pipe. 

The cable will be run through the pipeline to a point where the pipeline becomes exposed on the eastern side of the jetty located on Jetty Road at Moss Landing State Beach (see Figure 1). At this point, we will install an access hatch in the pipeline to pull the cable out of the pipe. 

MBARI is currently investigating the option of using Horizontal Directional Drilling (HDD) to drill underneath the channel of the harbor. The cable will then be brought onshore on MBARI’s property located on the southern side of the channel (see Figure 1). MBARI has contracted with Environmental Crossings, Inc. to provide a report detailing the HDD process. We will submit a copy of this report as soon as it becomes available. (As a side note, we have had preliminary meetings with California State Parks, who have indicated that they will likely be able to permit this activity.)

Once the cable is brought onshore on MBARI’s property, we will then trench alongside the roadway to bring the power in the MARS cable back to a currently existing structure (Building D) on MBARI’s main campus (see Figure 1). The fiber will be routed to Building D on existing overhead poles. Building D will then function as the MARS Shore Facility. The Shore Facility will include the shore power supplies, breakers, hubs, and other equipment necessary to feed power and communications to the observatory cable. 

Option 2 – Duke Energy Pipeline to Iso Van on MBARI Property
Option 2 will be the same as Option 1 until the cable is brought onshore on MBARI’s property on the southern side of the channel. For Option 2, the Shore Facility will consist of equipment housed in a 6-meter-long ISO van placed on MBARI’s property at the end of the island (see Figure 1). (An ISO van is a temporary structure typically used by scientists as portable laboratory space [see Photographs E-6 and E-7 in the original application packet]). 

Once the cable is brought onshore at this location, the power will be supplied from an existing power utility source. As in Option 1, the fiber will run along existing overhead lines to Building D on MBARI’s main campus.  

Option 3 – Moss Landing Marine Laboratories Pier
This option was formerly identified as the “Southern Shore Landing Alternative” and has not changed from the original application description, as listed here.  

For Option 3, the cable will run from a water depth of approximately 16 meters at the estimated position for the end of a planned pier to be constructed by Moss Landing Marine Laboratories (MLML) on the seaward side of the MBARI facilities. The estimated position of the end of the pier is 36(80.266' N, –121(79.111' W. Figure E-6 is a drawing of MBARI buildings and the planned MLML pier. Figure E-7 shows additional details. MLML has obtained permits to construct this pier and has given MBARI permission to land the MARS cable through conduit running alongside the pier (see Document E-2 in the original application binder). 

From the pier, the cable will run in the conduit and follow the same path as an existing seawater intake pipe before terminating in a circuit breaker box located inside MBARI Building C (see Figures E-6 and E-8 in the application binder). 

For this alternative, Building C will serve as the Shore Facility, so no additional structures will be needed. As in Options 1 and 2, the Shore Facility (Building C) will house all items necessary for cable and node operations including uninterrupted power supply and all command and control equipment. The existing power supply is sufficient to meet cable and node requirements (3 phase, 480-volt, 10kW).
Photographs E-9 and E-10 in the original application binder show views west and north, respectively across the proposed landing site (pier to be built) for the southern alternative shore landing.
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