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Engineering Lab

Rover to MARS Cable Pack Interface

Position Rover in proximity to MARS node

If Rover is within 20 meters of MARS Node, SIMM housing can be placed on seabed, and inter-connect performed with service loop.

If Rover is greater than 20 meters of MARS Node, SIMM housing will be placed within 20 meters of Node, and inter-connect performed with service loop.

Cable Handling Procedure;
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Step 1) Remove SIMM housing from cradle, place on seabed (less than 20 m) or transfer to ISE manipulator (more than 20 m)
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Step 2) Remove connector from dock and place on STAB on vehicle
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Step 3) Release Figure 8 of cable (pull up)
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Step 4) Release service loop, release lower shackles first (pull out)
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Step 5) Acquire service loop, grab is tie wrapped to shackle

                   Step 6) Proceed to within 20 m of node, place SIMM on seabed, remove grab from service loop and perform inter-connect, attach strain relief to node.
