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AWG 14 Conductor pairs shielded, If possible please solder to connector shell

Waterblocking (Cable Max?) present

Remaining conductors are #20AWG twp and will be used for data, twists should

be  maintained to solder cups as best as possible.

Jacket: Orange Polyurethane

Dia: 0.61"
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