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Depth

5000 meter 
Jacket Material


Moldable


Suitable for lay on sea bottom


Non-stick – talcum coated for shipping

Density in sea water


TBD – Gene to define

Torque


Neutral at depths 0 – 5000 meter
Minimum Bend Diameter


<18”

Conductors

Insulation



450 VDC rating minimum
Network pairs



Cat 5e – 2 pair required but could be 4 pair


100 Mb Ethernet traffic tested

List of tests

Power/signal conductors 


2x 14 AWG equivalent this is what I wanted for the PTT Craig


2x 20 AWG equivalent

2x 24 AWG equivalent – if 4 pair network cable used, this pair could be 1 of those 4 pairs.  If 2 pair network cable used, this pair needs to be added and needs to be twisted pair.
