MVC testing requirements
Equipment requested by Alcatel


See list


Major sticking point



Chroma DC electronic load



What did we use during the first test?


What other pieces of equipment listed are not available or need to be secured?

Software

New MVC has instrumentation that will be read by “Thomas”


Interface to the MVC will require integration into the MARS system at some point.

Safety


10kv testing during this operation



2 man rule in lab with 10kv energized



Restricted access to MARS lab




Alcatel engineer




Ed Mellinger




Ken Heller




Craig Dawe



All others require permission/supervision during testing phase


ERT response should be to the outside of the lab until power is secured and authorization from one of the above is given. Walk through of the electrical disconnects etc in the lab conducted prior to testing.

