MDUC 

September 17, 2002

1) CTD Salinity measurements 

Mike and Gernot

A year ago half of salinity measurements were off by more than 0.01.

Gernot and Mike have collected new data – salinity in water samples from rosette

Some sample trading with NPS – results agree within 0.001



Gernot recommends keep doing this for a while to establish validity. (at least through GOC expedition)



Using two sensors guarantees 0.01 accuracy. Collect samples routinely. Do water sample salinities whenever greater accuracy is required. 

Implication: core data is to 0.01, better accuracy requires project specific resources.

2) Oxygen Sensors

New SeaBird 43 is better than old SeaBird 13. Have two now to run on primary rosette – will use old sensors as spares on other platforms. Don’t need two sensors.

3) Core Proposals

4) ROV Navigation

