PCTD Table

Samples from the Shipboard Profiling CTD, chlorophyll and physical parameters (sensor data). One record for each meter in depth.

Owner: Tim Pennington, Mike Burczynski

Primary Keys: project, platform, expd, seq, depth

Field
Field Name
Type
Description

1
Pctd_ID
Integer
Internal Database ID number

2
Cruise
Text
Cruise name, i.e. S197, SU93-1, 00798

3
Expd
Integer
Expedition ID, JJJYY i.e. 15896 JJJ=Day of Year, YY= year

4
Seq
Integer
Cast number

5
Depth
Integer
Nominal depth sample was taken (meters)

6
Project
Character
Project Code

7
Ctrb_ID
Character
Internal Site Name

8
Platform
Character
Platform off of which the data were collected

9
Rjday
Integer
Running Jday from 1989 

10
date_time
Date
CTD cast begins sample collection

11
Jtime
Float
Time stamp

12
year_date
Integer
YYYYJJJ Year and Day of Year

13
dec_lat
Float
Decimal Latitude

14
dec_long
Float
Decimal Longitude

15
site_id
Character
Site Name

16
ctd_id
Character
CTD ID Number

17
Pressure
Float
Pressure sample was taken (dbar)

18
Tmp
Float
Temperature °C

19
Sal
Float
Salinity (psu)

20
Conduct
Float
Conductivity (volts)

21
Pot_temp
Float
Potential temperature  (°C)

22
Sigma_theta
Float
Sigma Theta (ml)

23
Parcos
Float
PAR cosine sensor (µE m-2 s-1)

24
par4pi
Float
PAR 4pi sensor (µE m-2 s-1)

25
Chla
Float
Calculated Chl  (mg m-3)

26
Fluor
Float
Fluorescence (volts)

27
trans_volts
Float
Transmissivity (v)

28
trans_pct
Float
Transmissivity (%)

29
trans_beam
Float
Beam C

30
oxy_ml
Float
Oxygen (ml)

31
oxy_ps
Float
Oxygen  (%)

32
OxyC
Float
Oxygen current

33
OxyT
Float
Oxygen temperature

34
Altimeter
Float
Operational Safety device, not loaded

35
IR443
Float
wavelength 443 (not loaded)

36
IR490
Float
wavelength 490 (not loaded)

37
IR555
Float
wavelength 555 (not loaded)

38
RDEP
Float
Real depth of cast

 

