
Microsoft Windows CE Ethernet Bootloader Common Library Version 1.1 Built Oct  1                                                                                
 2007 16:59:27              
Unlocking FLASH blocks.                       
INFO: LoadEBootCFG: Using default configuration for all blocks                                                              

Resetting factory default configuration...                                          

Resetting MemCfg oconfiguration...                                  

==================================================                                                  
 BitsyXb Platform - Bootloader                              
 ------------------------------------------------                                                 
 * Version 2.10               
 * SDRAM: 64 MB               
 * Flash: 32 MB               
 * Type: Retail               
 * Built on Oct  1 2007 at 17:04:17                                   
 * CPLD Rev: 6              
 * DIP SW: 1=off, 2=off                       
 * Boot Option: SEALED BOX UPGRADE                                  
 * Processor clock (turbo): 512 MHz                                   
==================================================                                                  

System ready!             
Preparing for download...                         
PC Cards Inserted: 1                    
 - ATA disk found. AtaDeviceIndex is 0                                      

Found resident NK image in FLASH:                                 
 - Copying to RAM... Done.                          

Jumping to image at 0xA0200000(P):0x80200000(V)...                                                  


Windows CE Kernel for ARM (Thumb Enabled) Built on Jun 24 2004 at 18:25:00                                                                          
ProcessorType=0411  Revision=7                              
sp_abt=ffff5000 sp_irq=ffff2800 sp_undef=ffffc800 OE                                                   
System DRAM (MB) - Total:64 Extension:None                                          
Sp=ffffc7cc           
Datalight FlashFX Pro v1.11 Build 856                                     
Copyright (c) 1993-2004 Datalight, Inc.                                       
Patents: US#5860082, US#6260156.                                
FFX: B1A00000 = CreateStaticMapping( 01A00000, 00600000 )                                                         
FlashFX SDK License ID #5B2C08D8                                
Created Thread E3C3EFD6                       
Datalight Reliance v1.13.0337                             
Copyright (c) 2003 - 2005 Datalight, Inc.                                         
Registered to #6A48B493                       
Initializing Debug Log Driver...                                
Failed      
Initializing FLASH Driver... FSHDRV: B0000000 = CreateStaticMapping( 0, 2000000                                                                               
) 
MfgCode 890089              
ok  
Initializing ADSLOAD.REG Parsing driver... ok (439ms)                                                     
Initializing POWER Driver... ok                               
Initializing Ethernet Driver...  Detected Ethernet(SMC91C111)                                                             
Ok  
OID_PNP_CAPABILITIES Statistics Query                                     
OID_PNP_CAPABILITIES Statistics Query                                     
Initializing SMARTIO Driver...                              
 SMARTIO Detected : PartType=0x8535 Firmware=0x0010 Revision=6                                                              
 SMARTIO : SerialClockRate=10 KBits/S(0xa7).                                            
ok  
Initializing Serial(driver version support IR)... UART0 ok. (107ms)                                                                   
Initializing Serial(driver version support IR)... UART2 ok. (107ms)                                                                   
Initializing Serial(driver version support IR)... UART1 oInitializing USB HCD...                                                                                
 Ok   
Initializing USB Client... Ok                             
Initializing I2C driver v 1.1...ok (1ms)                                        
USB HCD wakeUpThread: Read Registry setting error, use default value.                                                                     
Initializing Digital I/O Driver v. 2.2...ok (5ms)                                                 
Initializing WAV device... Ok                             
Initializing SDHC Driver... Ok                              
Initializing PXA25x Display Driver (v1.2)... Ok (364ms)                         
Initializing Touch Panel driver v 1.6... Ok (5ms)


   Microsoft Windows CE Ver. 5.0 (build 0)

   Windows CE Ver.(5.00.36 BX270_Pro_HIVE)
   Bootloader Version 2.10
   ADSLOAD.HWT Version 0x00000000
   ADSLOAD.REG Version Not Available
   CPLD Version 6
   AVR Version 10 6


   FlashFX Disk Size (5MB) OK


* ADSLOAD.EXE(do-nothing build): Complete
Current time
16:22:01
Delay value: 60,  Sleep value: 30000
Run at time
16:23:01
Notification handle: 0x0000012a
