Jim
Here you go.

1) The sketch is looking at the component side of the proto board.  The side with the 240 tiny weenie pads.

2) The notch in the corner of the proto board is to clear the corner of a connector on the computer board.

3) The odd numbered pins need to be on the notch side of the proto board.

4) You need to leave at least 7 pads on the right side of the proto board (the notch side) empty so that the proto board will stick out far enough to allow me to put a standoff into the existing hole on the computer board.

5) The very edge of the proto board on the side of the connector with the even pin numbers will be near the inside wall of the pressure housing so it would be best not to use holes near that edge.  I tried to lay out the connector pin number vs which row of plated through holes they use on the Excel spread sheet.   The print out shows what happens with 7 unused pads on the right of the connector.  It looks to me like we would be better off leaving 9 unused pads on the right of the connector since that means you can put the pins on the ground pads on the odd numbered pins.  But you should check this to make sure.

6) Feel free to look at the computer board in my office if that helps.

7) I’ll try to be in between 0730 and 0800.

Thanks - Gene

