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Purpose

This project will record acoustic measurements of mass sediment transport events in the Monterey Canyon.  Estimates of the duration and nature of these events can be inferred from the acoustic records.  Detection of sediment transport events will be triggered by the STEDs used in the ongoing Canyon Dynamics project.
Methods and Equipment

A simple, battery powered hydrophone and data logger will be used to make the acoustic measurements.  We envision this package to be roughly 1m x 0.5m x 0.5m.
Sanctuary Prohibition

There are minor seafloor alterations when the package is deployed and recovered. Deployment sites rapidly fill in with new sediment, and the seafloor is returned to the original state quickly. 

Plans for 2008
Two deployments are planned for 2008.  One will be a 1 day test deployment and the second will be a 90 day deployment. 
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