Adaptive Modulation Data Sheet

One or more paths in this Data Sheet use microwave radios with Adaptive Modulation. These paths can be identified by a numerical superscript notation immediately following the Radio Code on the path data sheet.

The superscript notation can be cross referenced to the corresponding table(s) below to identify the various modulation modes in which the microwave path will operate.

(1) Master Radio Code: X18147 - EXALT COMMUNICATIONS INC.	
Pages: 1	
Radio Code	Model	Model Description	Emission Designator	Modulation	Loading (Mbps)	Stability (%)	Coordinated Power (dBm)	
TEPA49	E18F732-1560X1-256Q-30MHZ	EXTENDAIR G2 RC18020	30M0D7W	256 QAM	1 CH DIG 196.0	0.0007	19.0	
TEPA53	E18F732-1560X1-128Q-30MHZ	EXTENDAIR G2 RC18020	30M0D7W	128 QAM	1 CH DIG 171.0	0.0007	19.0	
TEPA59	E18F732-1560X1-64Q-30MHZ	EXTENDAIR G2 RC18020	30M0D7W	64 QAM	1 CH DIG 147.0	0.0007	19.0	
TEPA69	E18F732-1560X1-32Q-30MHZ	EXTENDAIR G2 RC18020	30M0D7W	32 QAM	1 CH DIG 122.0	0.0007	19.0	
TEPF33	E18F732-1560X1-16Q-30MHZ	EXTENDAIR G2 RC18020	30M0D7W	16 QAM	1 CH DIG 98.0	0.0007	19.0	
TEPF37	E18F732-1560X1-4Q-30MHZ	EXTENDAIR G2 RC18020	30M0D7W	QPSK	1 CH DIG 48.0	0.0007	19.0