 
In order to change the TR Space you will need to do the following-
 

Log in as factory
 

Username:- factory
Password:- arct1c
 

Go to :-
1] Analysis
2] ODU Trace
 

<enter the following >
 

pass cbjc
 

<send command>
 

trspace -50    ("or what ever you number is please note to have a space after trspace and the number is MHz")
 

<send command>
 

Tx  6512.5  ("or what ever your frequency is ")
 <send command>
 

 

Rx 6462.5  ("or what ever your frequency is ")
 

 

<send command>
 

 

 

Then power cycle  unit.
 

