 
Moseley EventHD Manual Config.

 

 

Log in as factory

Username:- factory

Password:- arct1c

 

Go to:

1] Analysis

2] ODU Trace

 

<Enter the following >

 pass cbjc

 <send command>

 

trspace  50    ("or what ever you number is please note to have a space after trspace and the number is MHz")

 <send command>

 

Tx  6512.5  ("or what ever your frequency is in MHz")

 <send command>

  

Rx 6462.5  ("or what ever your frequency is in MHz ")

 <send command>

 

  

Then power cycle  unit.

 

You can select HT/LT (high or low transmit) in the GUI if you first enter "TXRELAY 1" into the ODU Trace terminal. Or you can set it in the ODU Trace terminal by using the TXBAND < HI | LO > command (select either HI or LO). You can read the current state by entering only TXBAND.  

 

In order to get these settings to stick after an IDU reboot you will want to set TXBAND, TX, RX, and TSPACE then navigate to Administration -> Maintenance and then perform an East Modem reboot. Once this is performed you will only need to return to ODU Trace to change TRSPACE. The HT/LT selection as well as the TX freq can be selected during a link configuration process. 

 

Commands:

trspace  XX
Freq in MHz 
tx XXXX.X
Freq in MHz

rx XXXX.X
Freq in MHz

txband XX
HI/LOW
