Uploading Instructions:

 

You will also need an FTP client program on that computer to upload the file to each IDU. Filezilla or FireFTP are free open source programs that are effective FTP clients for this procedure but other FTP client programs will work.  

 
1. Put this modes.img file on the computer that is connected to the IDU. 

2. Open your FTP program and log into the IDU to be upgraded with the username “integrator” and password “p1nacate”. 
3. Copy the “modes.img” file from your local computer to the IDU directory. 

4. Next, open a web browser on your computer. Enter the IDU’s address in the browser address bar. The browser will request the username and password before bringing up the IDU’s web interface. Use the same username “integrator” and password “p1nacate”. 

5. From the web GUI left navigation panel go to Administration -> Maintenance -> Reprogramming screen. 

6. Select the “MODES” check box and click the toggle button. You should see the green dot adjacent to the M1-11v2 mode showing that it is selected. 

7. From the web GUI go to Administration -> Maintenance -> Reboot. 

8. Select the IDU check box and click the reboot button. 

9. It will take the unit a couple of minutes to reboot. 

10. Select the newly available modes from the web GUI left navigation panel under Link Configuration -> Radio Link -> Link Configuration 

11. Follow the Link Configuration wizard through all steps and select “update all”. 

12. Repeat the above steps for the 2nd IDU. After rebooting the radios should lock up and you should see a green LED on the modem on each IDU. 

 

Note: The procedure must be repeated for both IDUs. The same mode must be loaded to both IDUs and be similarly configured for the link to operate correctly.

