Firmware Upload Procedure

1) First connect computer/laptop RJ45 port to either encoder or decoder using a crossover cable.

2) Then confirm the IP address of the encoder or decoder by selecting control/network/IP address/

3) Once the IP address is confirmed you must change the IP address on the computer to match the sequence of the IP address set on the encoder or decoder. 

Example: 

Encoder IP address: 192.168.001.101      Subnet Mask: 255.255.255.0 (class A)

Change computer IP address:

Computer IP address: 192.168.001.100     Subnet Mask: 255.255.255.0 (class A)

   Once the IP address is changed you must access the encoder or decoder from the computer by typing IP Address and extension.

    Example:   http://192.168.001.101/update.htm

4) User: admin

Password: none

5) Type password 14142135   hint: square root of 2, the first eight digits.

6) Click browse buttong and select firmware version. Remember load firmware that is specific to encoder or decoder.

7) Wait for firmware to be loaded and process to be complete on both encoder/decoder and computer. (Must be very careful not to disrupt units during this process as it may crash the encoder or decoder.

8) When process is complete power cycle the encoder or decoder. Once the unit is ready, go ahead and confirm that the current firmware is loaded by checking the firmware on the front panel.  You can view this by selecting Version – Main – Firmware.

