2008.10.20
NTT Electronics Corp.
HVE9100 Version & Contents
	Version
	The main contents of revision

	Integration
	Download
	Base
	

	01.00
	01.00
	01.00
	First release

	01.50
	01.50
	01.00
	1) Fixed the bug of BISS interconnectivity with the other company’s decoder.
2) Added the function of video filter.
3) Changed the upper limit of video bit rate.(HD:80Mbps, SD:40Mbps)
4) Support 1920x1080I: M=1.
5) Fixed the bug that the video output is frozen when a complex video image is input, and improved the quality of video output.
6) Fixed the bug that pulled out and opened the external clock caused system reset.
7) Fixed the bug that the external clock of 10Mbps or less is not detected.
8) Fixed the bug that the matrix of input audio is reset when the SDI input is pulled out and opened.
9) Fixed the bug that the first item of the log is deleted.
10) Fixed the bug of color shift.

	02.00
	02.00
	03.00
	1) Addition of video format 1080I25, 720P50, 720P59, 720P60, 576I25.
2) Fixed the bug that a normal Ancillary packet might not be output when the ancillary packet set with the encoder is not input.

3) Addition of TS over IP. (optional)
4) Addition of audio channel.(+8ch)  (optional)
5) Improved the quality of video.
6) Addition of AES and Embbeded coexistence setting.

7) Addition of MPEG2 BC audio. 
8) Addition of 4PES MPEG1 audio.

9) Addition of MPEG1 (mono/dual-mono)audio. 
10) Addition of AAC (1ch(mono),2ch(dual-mono),4ch(2/0x2),6ch(2/0x3))audio.
11) Shortening of TS stop time when MPEG1 (mono / dual-mono /stereo) is switched. 
12) Shortening of TS stop time when AAC (mono/dual-mono/stereo) is switched. 
13) Addition of video format for SMPTE334M.
14) Addition of ancillary user definition data.
15) Addition of ancillary defined in ARIB Standard.

16) Addition of external LTC. 
17) Correction of the threshold value of a temperature sensor. 
18) Addition of event trap, with abnormal temperature and abnormal FAN, etc. .
19) Addition of preset parameter download/upload. 
20) Addition of NIT and SDT.
21) Addition of TRAP customize. 
22) Addition of NIT, SDT and Device information in MIB.

	02.20


	02.20
	04.00
	1) Changed the upper limit of video bit rate for CABAC.

	02.50
	02.50
	04.00
	1) Addition of Low latency mode.
2) Improved the quality of video.

3) Changed the upper limit of video bit rate for CABAC.

4) Changed of embedded audio error detection.
5) Addition of protecting preset parameter.

6) Changed of the format of Audio mode menu.

7) Addition of 4:2:0 version.

8) Fixed the bug that video data is not output when the device start up.

9) Fixed the bug that the error occurred if “Param Select Mode” and “Null Output Mode” are used at the same time.
10) Fixed the bug of “IIC BUS ERROR” when the alarm event occurred frequently.

11) Fixed the bug that the some event log is erased when recorded time is wrong.

12) Changed that Ancillary, TS over IP, BISS are included in the presetting parameter.

13) Fixed the bug that IP output setting is not normally done by SNMP.

14) Fixed the bug that the port number for IP output cannot be set smaller than 6000 by SNMP.
15) Fixed the bug that Web password is overwritten when SNMP setting is applied.


Notes 1. "an integrated version" is the version for management included to mechanisms, such as a case of equipment, and internal wiring.
Notes 2. "a download version" can be checked by the version display of an equipment operation menu, and builds main encoder ability, such as PLD/firmware. 
Notes 3. "a base version" shows versions, such as a monitor program for firmware starting for control.

































