Help

Barix constantly enhances the capabilities of their products. Therefore we recommend to keep the software on the device up-to-date.
To download the latest firmware version please visit www.barix.com.
Download the firmware update package and unpack to a local drive.
Updating files
Click on "Please click here to continue" to launch the update process.
Before you click the link note that the update process can only be canceled by power cycling the device.
The device will restart in a special mode called Bootloader and a screen appears showing a number counting down.
To upload an update click on "Browse..." to locate the file you want to update.
Once selected, click on "Upload".
This process can take a few minutes.
After a successful upload the following text appears:
"Resource" successful loaded. Click on update before updating the next component or unplug power supply to reboot the device.
Click on the update link before updating the next component. Unplug power supply to reboot the device or type "reboot" in the resource field and click on "Upload".
A screen stating "rebooting" appears.
Close the browser window. After the device has rebooted open a new browser window to continue.
Version display
Versions are displayed on the right hand side of the Barix logo.
MAC shows the MAC address of the device.
Firmware version shows the current version of the Firmware.
Web application version shows the current version of the Web application.
Bootloader version shows the current version of the Bootloader.
Setup version shows the current version of the Setup.