&L(0,"*",21);

SETTINGS &LSetup(3,"%s",130,D,0,"");

NETWORK | AUDIO | STREAMING | I/O | CONTROL | SERIAL | SECURITY

Own Name |
Streaming mode |
Trigger Level | only for mode "send on Level"
Pre Trigger Start | msec
Post Trigger Play | msec
Buffer Underrun Mode (TCP) |
Background Stream TCP Flow Control |
Stream Packet Strategy (MP3 only) |
Non MP3 Packet Size | Bytes
Play Buffer | Bytes
Receive Timeout | msec
TCP Priority Rx Port |
UDP Priority Rx Port |
Minimum Priority Message Volume | %
UDP Receiver Port |
UDP Tx Source Port |
Radio Path |
Relay While Audio |

Stream | from table to origin source
Table | 1 2 3 4 5 6 7 8 | Current Table &LState(3,"%u",46);

SNMP
Trap Target IP Address | . . .
Low Audio Level | Left | Right
High Audio Level | Left | Right
Trap Repeat | Left sec | Right sec
Silence Timeout | Left sec | Right sec
| &LSetup(3,"%s",122,D,!0," Save Config Password ");