Help

Here you can configure the device's Static IP address. With this you can set a permanent IP address so that the device does not have to get a new one upon power-up. We recommend that you set a Static IP address.
IP Address
Enter the 4 values of the desired device IP address e.g.:
"0.0.0.0" for automatic discovery (DHCP/Bootp, IPzator, AutoIP)
"192.168.0.12" for an internal LAN
Default: "0.0.0.0"
Netmask
Enter the 4 values of the desired Static IP e.g.:
"0.0.0.0" for a default Netmask depending on the IP Address used.
"255.255.255.0" for a C class network
Default: "255.255.255.0"
Gateway IP Address
Enter the 4 values of the desired Gateway IP address e.g.:
"0.0.0.0" for no Gateway
"192.168.0.1" for a Gateway in a LAN
Note: The Gateway has to be set only when connecting to other devices over the WAN (through a router).
Default: "0.0.0.0"
Use SonicIP®
If set to "yes", the device will announce its IP address over the audio output.
Default: "yes"
To store these settings click on "Apply".
The device will restart with the new setting.