Help

This page shows the status of the device.
Several links allow control and allow simulation of button inputs, relay output and control signals of the serial port.
The manual and the technical documentation is available on www.barix.com.
Status
Shows the current status. The nearby button refreshes the status information.
Possible states: "INACTIVE", "TALKING", "TALKING SUPPRESSED", "FORCED TALKING", "LISTENING".
Input and Output peak level
Shows the peak level of the audio input (Line in or Mic In) or audio output respectively. The value shown is in linear scale from 0 (silence) to 32767 (full scale signal).
TALKING
Click the "FORCE" link to force the talking (not visible if "send always" mode is configured). This overrides the "TALKING SUPPRESSED" mode, e.g. when other device is talking to this device.
Click the "TALK" link to start talking (not visible if "send always" mode is configured).
Click the "STOP" link to stop talking (not visible if "send always" mode is configured).

The indicator next to TALKING has the following meaning:
  - not talking
  - talking
  - forced talking

TABLE
Select the streaming table by its number.
ENTRY
Select "All" for talking to all configured entries within the table. Select a particular number to talk only to that entry.
BUTTON 0 and 1
Shows the status of and controls the button inputs.
Click "SET" to simulate button beeing pushed, click "CLR" to simulate the button beeing released.

The indicator next to "BUTTON" shows the status of the physical input (simulation is not shown!):
  - button released (input not activated)
  - button pushed (input is activated)
  - shortcut on the input (available only on devices supporting supervision)
  - no connection (available only on devices supporting supervision)

RELAY
Click the "PULSE" link to activate the relay for the "Relay pulse duration" time, adjustable in "Settings" under "I/O".
Click the "SET" link to activate the relay.
Click the "CLR" link to deactivate the relay.

The indicator next to "RELAY" shows the physical status of the relay:
  - relay not activated
  - relay activated

CTS IN (RS-232)
Click the "SET" link to simulate CTS beeing activated.
Click the "CLR" link to simulate CTS beeing deactivated.

The indicator next to "CTS IN" shows the physical status of the CTS (simulation is not shown!):
  - not activated
  - activated

RTS OUT (RS-232)
Click the "SET" link to activate RTS.
Click the "CLR" link to deactivate RTS.

The indicator next to "RTS OUT" shows the physical status of the RTS:
  - not activated
  - activated

MIC
This field is available only on devices supporting supervision. Shows the status of the microphone:

  - microphone detected and operating properly
  - microphone not attached or shortcut detected

TEMP
Shows the device's internal temperature in degrees centigrade. The information is available only on devices supporting supervision.
Tips
- To configure the device click on the "CONFIGURATION" button.
- The white triangle next to the Annuncicom IC logo as well as the "+" (above) and the "-" sign (below) can be used to change the volume temporarily.
- This page can be customized to meet installation requirements. Download the development kit from www.barix.com.