Help

These settings adjust the control port properties.
UDP command port
Defines the port where the device will receive commands via UDP. To disable set this port number to "0".
Default: "12301"
TCP command port
Defines the port where the device will receive commands via TCP. To disable set this port number to "0".
Default: "12302"
Web server port
Defines the port where the webserver of the device can be reached. If set to "0" the default HTTP port (80) is used.
Default: "0"
Serial Interface 1
Define the functionality of the 1st serial interface. "Command Interface" means the interface is used to input commands. "Keypad" disables the serial command interface and supports a keypad.
Default: "Command Interface"