&L(0,"*",21);

SETTINGS &LSetup(3,"%s",130,D,0,"");

NETWORK | AUDIO | STREAMING | I/O | CONTROL | SERIAL | SECURITY

Command Broadcasting |
Init Sequence |
I0 pushed command |
I0 released command |
I1 pushed command |
I1 released command |
Relay pulse duration | x 0.1 sec (Door buzzing duration)
CTS close command |
CTS open command |
RTS pulse duration | x 0.1 sec
| &LSetup(3,"%s",122,D,!0," Save Config Password ");