Help

These settings adjust the device behavior for startup, inputs and outputs (attached buttons, the serial CTS signal and the relay pulse duration).
Command Broadcasting
This option is for backward compatibility with firmware versions prior to 1.16. If you want "r=c=" commands to be broadcast (UDP broadcast), set to compatibility mode. Otherwise choose secure mode, then "r=c=" commands will be sent only if stream to origin source is set and the origin source is known (command will be sent to the last partner).
Init Sequence
This command sequence is always executed immediately after startup (see further below for commands).
Default: ""
I0 pushed command
Configure which command should be issued when the I0 button is pushed (see further below for commands).
Default: "c=83"
I0 released command
Configure which command should be issued when the I0 button is released (see further below for commands).
Default: "c=84"
I1 pushed command
Configure which command should be issued when the I0 button is pushed (see further below for commands).
Default: "r=c=78"
I1 released command
Configure which command should be issued when the I0 button is released (see further below for commands).
Default: "r=c=79"
Relay pulse duration
Defines the amount of time (in tenths of a second) the door strike will buzz when the "Dout" pulse command is received.
Default: "30" (3 seconds)
CTS close command
Configures which command is issued when the CTS signal on the serial connector is activated (see further information below in the command description).
Default: "r=c=78"
CTS open command
Configures which command is issued when the CTS signal on the serial connector is deactivated (see further information below in the command description).
Default: "r=c=79"
RTS pulse duration
Defines the RTS pulse duration (in tenths of a second) when the "RTS" pulse command is received.
Default: "0"
Commands
Multiple commands can be added using the & character. They will be executed sequentially in the order that they appear in the configuration field.
TALKING MODE
c=83 : Activate the talking mode
c=84 : Deactivate the talking mode
c=91 : Activate the forced talking mode
STREAMING
c=77 : Set destination Syntax : c=77&entry=x&ip=a.b.c.d&port=p&type=t
For x use 1 to 8 (Streaming destination 1 to 8)
a.b.c.d is the IP address to stream to
p stands for the port number to be used
For t use 0 (not used), 1 (Raw UDP) or 2 (Raw TCP)
Example:
c=77&entry=2&ip=192.168.0.100&port=3030&type=1 sets the destination 2 to Raw UDP to IP 192.168.0.100 on port 3030
I/O
c=78 : Activate the relay
c=79 : Deactivate the relay
c=80 : Pulse the relay for the preset time
c=85 : Simulate the I0 button being pressed
c=86 : Simulate the I0 button being released
c=87 : Simulate the I1 button being pressed
c=88 : Simulate the I1 button being released
SERIAL
c=89 : Simulates the CTS Signal being activated
c=90 : Simulates the CTS Signal being deactivated
c=60 : Activates the RTS Signal
c=61 : Deactivates the RTS Signal
REMOTE COMMANDS
r=x : send the command x to the last calling station remotely
r=a.b.c.d:p/x : send the command x, using UDP, to the remote IP a.b.c.d on the optional port p. Default if no port is defined is the configured UDP command port.
Example:
r=192.168.0.99:12301/c=83 (sets the remote station to talking mode)
For further commands refer to the technical documentation available on www.barix.com.