0116
/* * * * * * * * * * * * * * * * * * * * * * * * * * *
Vers  Date     Who  What
00.01 10.05.07 PK - initial revision
00.02 15.05.07 PK - on/off states swapped
00.03 16.05.07 PK - hardware detection added (BCL_IO_INIT call)
                  - analog values: voltage+temp
		  - PIC control
00.04 17.05.07 PK - save/restore PIO registers for the case when autodetection fails
00.05 12.09.07 PK - added support for the new PIC firmware for Ann1000 (9-bit voltage)
00.06 03.10.07 PK - hardware detection added, driver structure changed, separate driver for each hardware type
                  - EX1000 driver added, I2C driver from song added
      12.10.07 PK - structure rewritten to fit the new song driver architecture
      24.10.07 PK - Ann1000 driver split into several modules to allow usage by song
                  - PIC control register in Ann1000 driver moved into shared memory (int vector 26h)
                  - fixed bug in restore PIO where the pins were set to "normal operation" which could cause a crash
00.07 31.10.07 PK - digital output and relay toggle added
                  - digital output and relay pulse function added
		  - generic IO driver for standard Annuncicom, Exstreamer, Instreamer
      01.11.07 PK - RTS/CTS functions on all hardware
      02.11.07 PK - corrected the default RTS value for LX hardware
                  - added full control of the Annuncicom 1000 hardware
		  - Bosch/Annuncicom 1000 detection
      05.11.07 PK - fixed null-pointer dereference bug when no driver found
      06.11.07 PK - voltage and temperature on Ann1000 in 0.01 units
      07.11.07 PK - generic driver: added support for EX110 relay
      08.11.07 PK - ann1000: fault relay inverted
                  - ann1000: fixed reversed numbering of inputs
      09.11.07 PK - generic driver: removed unnecessary code
00.08 09.11.07 PK - IPAM driver added
                  - corrected inverted RTS on second serial
00.09 14.11.07 PK - display interface added
                  - display driver for ST7036 (EX110)
		  - backlight control
      15.11.07 PK - 7-segment display driver added
      21.11.07 PK - display scrolling 
                  - display clear block
      22.11.07 PK - octal character notation (\123) support added into display driver
00.10 24.01.08 PK - Barionet V2 driver added
      25.01.08 PK - hardware type in little-endian
00.11 03.02.08 PK - DS6 console driver added
      04.02.08 PK - added support for ANSII escape sequencies to the print function
00.12 05.02.08 PK - keyboard support
                  - keyboard driver for DS6 MTSD
      11.02.08 PK - Digigram decoder driver added
      12.02.08 PK - Digigram: PIO reassignment
                  - Digigram driver: input bug fixed
      05.03.08 PK - fixed bug in 7-segment display detection
00.13 25.03.08 PK - hardware detection based purely on ee_hw_type - WILL NOT WORK IF TYPE NOT SPECIFIED!
00.14 17.04.08 PK - stack size of the IO process increased from 200 to 300
      18.04.08 PK - Digigram hardware type changed from the temporary type to a real value
      21.04.08 PK - bugfix #018.04: Ann 1000 driver: LEDs should not blink
      21.04.08 PK - temporary hardware type for Digigram put back in
      08.05.08 PK - more secure LED control: noise in input shiftreg can not change the control pins
00.15 09.07.08 PK - added hardware descriptor from IO port 60000 (read using IOSTATE)
      23.07.08 PK - intial version of Barionet LC driver
      19.08.08 PK - fixed non-working LF in display print function
00.16 22.08.08 PK - initial support for PYKO IN/FD
      27.08.08 PK - PYKO IN/FD driver: MUX control moved to song
      19.09.08 PK - iostate(60007) returns the number of keys
                  - Ann1000: inputs 1..8 can be scanned as keyboard events
                  - Ex1000: inputs 1..4 can be scanned as keyboard events
      20.09.08 PK - Ann100/200: inputs 1..2 can be scanned as keyboard events
                  - Pyko: inputs 1..4 can be scanned as keyboard events
      26.09.08 PK - DS6 driver: added hardware type detection
                  - LED control via auxilliary control interface
      27.09.08 PK - fixed IOCTL pulse bug on IO 200
      29.10.08 PK - increased stack size to 500B
      13.11.08 PK - assigned hardware type for Barionet 50
00.17 21.11.08 PK - harris display driver rewritten
                  - separate driver for 7-segment displays
		  - initial version of VSC display driver
00.18 22.11.08 PK - new interface to io_init - all parameters are in one structure
      29.11.08 PK - initial support for VSC
00.19 02.01.09 PK - added DILL - display interpreted language library, a programmable display library
      06.01.09 PK - driver reports to the application if the standard LEDs are used
      20.01.09 PK - improved VSC communication for better data synchronisation
00.20 21.01.09 PK - interface simplification: removed display_gotoxy and display_clear calls
                    use display_print with an appropriate ANSI sequence instead
                  - removed display_message call- use DILL instead
		  - removed display_print_flash_file_entry - use DILL instead
      26.01.09 PK - second display support, so far can be used only with DILL
00.21 04.02.09 PK - enabled PIO17 on the IPAM carrier board
      06.02.09 PK - feature request #018.16: enabled access to PIO11, PIO17, PIO29 and PIO30 on IPAM 200/Exstreamer 100
      12.02.09 PK - PS16: increased the maximum number of extensions to 5, 
                    but only 2 will work with key events and only 1 can be used with IO map
		  - Barionet 50: updated driver to the latest schematics
      13.02.09 PK - Barionet 50: 1-wire temporarily mapped to IO 101
      27.02.09 PK - PS16: the number of supported keys limited to 100

01.00 18.03.09 PK - IR handler moved from song to bclio
                  - ignores hw_type from the init call and uses get_hw_type() call instead
      19.03.09 PK - added IR_READ_HIGH_LEVEL call
      20.03.09 PK - IR decoder: added various formats into the high level decoding routine
      06.04.09 PK - Exstreamer 1000: LEDs were inverted (input inactive - LED was on), fixed
01.01 04.05.09 PK - started 1-wire driver implementation
      02.06.09 PK - Barionet50: digital input logic changed to positive (negative before)
      05.06.09 PK - added 1-wire RTC driver
                  - Barionet 50: temperature sensor addresses mapped onto IO 651-700
		  - added 1-wire driver for DS18B20 temperature sensor family
		  - Barionet 50: temperature sensor measurement on registers 601-650
01.02 08.06.09 PK - exported 1-wire interface
      09.06.09 PK - 1-wire discovery algorithm rewritten
                  - added 1-wire RTC interface
		  - 1-wire support in Ex1000 and IPAM
		  - built-in TS support on Ex1000
      10.06.09 PK - 1-wire processing rewritten to asynchronous with request queueing
                  - implemented calls for RTC read and set
      12.06.09 PK - created another build target bcl_io_x with extended tables (for Barionet 50)
01.03 13.06.09 PK - implemented virtual bits 301..400
      15.06.09 PK - Barionet 50: implemented virtual word registers 701..1000
                  - Barionet driver excluded from bclio.bin to save space
		  - Barionet 50: implemented 32-bit counter registers 
		  - Barionet 50: RTS control on IO 9 rather than IO 200
      16.06.09 PK - Barionet 50: virtual relays and digital outputs implemented
      17.06.09 PK - Ex1000: non-working temperature measurement fixed 
      22.06.09 PK - DILL: get_int and 'I' rewritten to support signed
                  - bugfix #065.01: output/relay pulse changed: sets immediately in ioctl, the pulse can be 10ms inaccurate
01.04 22.06.09 PK - feature #018.21: PS16 driver: supports up to 112 keys (2 complete extensions)
      23.06.09 PK - LED control: show inputs, show outputs, map as digital outputs in the IO map
                  - Ann1000: simplified driver, full LED control, LEDs mapped to IO 151-158 (if enabled)
      24.06.09 PK - Ex1000: full LED control, LEDs mapped to IO 151-154 (if enabled)
      27.06.09 PK - DILL: 'i' integer variables are signed; added variable type 'u' for unsigned integers
                  - DILL: added % operator
		  - DILL: nice called after every command
      08.07.09 PK - PS16 driver: fixed wrong polarity of LEDs in iostate
      09.07.09 PK - PS16: keyboard scan period increased from 3ms to 10ms
      16.07.09 PK - Ex110 display driver: wait 4ms after clear screen instead of 2ms
      28.07.09 PK - added RDI556 serial RTC driver
                  - Barionet50: 1-wire RTC enabled only if no serial RTC attached
      30.07.09 PK - added IO_AUX_SET_IO_MASK
01.05 03.08.09 PK - added IR_FORMAT_CMD into the high-level IR function, which returns directly the command to be executed
                    this dramatically simplifies the IR process in the application
      07.08.09 PK - external 1-wire enabled for Barionet 200
      13.08.09 PK - 1-wire: fixed non-portable inline assembly use, which did not work with -k- option (bug #066.03)
01.06 27.08.09 PK - implemented virtual 16-bit registers 501..600 on Barionet 50 (feature #064.08)
      01.09.09 PK - virtual 16-bit registers in bcl_io.bin (ABCL) (bug #047.23)
      04.09.09 PK - special target for ABCL: bclio_a.bin; virtual 16-bit registers removed from the standard version bclio.bin
01.07 05.09.09 PK - added IO subscription mechanism in Barionet 50 driver
                    WARNING: init incompatible with previous versions
      11.09.09 PK - changed interface to IO subscriptions: multiple subscriptions possible
      23.09.09 PK - fixed wrong number of relays and digital inputs on Barionet50 (bug #064.18)
                  - fixed non-existent analog values on Barionet 50 (#064.19)
01.08 07.10.09 PK - output pulse and toggle slightly modified:
                  - toggle only by ioctl x,999 (before it was any value >=999)
		  - toggle, set or reset stops already running pulse timer
		  - fixed bug in pulse function: total count was wrong if pulse repeated
		  - added IO_PULSE_TOGGLES compile option for Barionet compatible behaviour of the pulse function (#064.24)
      15.10.09 PK - 1-wire TS: measurement time increased from 760ms to 1s (as a precaution against bug #064.17)
		  - 1-wire TS: fixed wrong timing of high-power in a "send, high power" sequence (bugfix #065.02)
      16.10.09 PK - bugfix #064.17: 1-wire collision with the RS485 port (CTS) resulting in temp sensors always reading 0
01.09 10.11.09 PK - Ex1000 temperature sensor disabled because it was disturbing 44kHz PCM audio FDX (bugfix #048.09)
01.10 08.12.09 JP - bugfix #047.19: device resets if DHCP server responds too quickly
                    caused by nice() within enable/disable chip select in Ex110 display driver (pin shared with the reset button)
01.11 17.12.09 PK - feature #047.33: added support for reset button as a digital input (IO address 296) 
01.12 28.12.09 PK - initial version of the Ann155 driver
      31.12.09 PK - Ann155: fixed wrong order of digital inputs
                  - LED output mapped as a relay rather than digital output
      06.01.10 PK - Annuncicom 1000 PIC driver: delay before data reception increased from 3us to 10us (for compatibility with Ann155)
      12.01.10 PK - bugfix #064.43: 1-wire reports temp value 0 even if bus is shorted
                  - bugfix #064.51: temperature sensors are not in subscriptions
      05.02.10 PK - bugfix #064.43: 1-wire reports temp value 140.6 if bus is shorted
01.13 25.02.10 PK - #065.05: Annuncicom VME driver
01.14 21.04.10 PK - #065.06: Exstreamer 120 support
01.15 19.07.10 PK - #065.08: added support for Exstreamer 500
      20.07.10 PK - Ex1000: LED update and input scanning frequency reduced from 100Hz to 20Hz to reduce system load (bug #61.10)
01.16 29.07.10 PK - #055.21: Annuncicom 155: negative temperature displayed improperly
                  - #065.09: added speaker supervision support for Annuncicom 155
*/
