&LSetup(3,"%s",130,D,0,"");

BASIC SETTINGS |

NETWORK SETTINGS |
Use SonicIP | Yes No
IP Address | . . .
Netmask | . . .
Gateway IP Address | . . .
Primary DNS | . . .
Alternative DNS | . . .
Syslog Address | . . .
DHCP Host Name |
Web Server Port |

OUTGOING STREAM |  |
--- | --- | ---

Stream Method | URL | Port

Streaming Mode |
Input Trigger Level |
Input Inactivity Timeout | msec

Output Trigger Level |
Output Inactivity Timeout | msec

Keep-alive Period | msec

INCOMING STREAM |  |
--- | --- | ---
Stream Method | URL | Port

RTP delay |

AUDIO |

Format |

Sample Rate |

Quality |

Input Source |
Input Gain | dB

Output Audio Level | dB

Fading Effect | Enabled Disabled

I/O AND CONTROL |
Front Panel LEDs |

Relay 1 Mode
Relay 2 Mode
Relay 3 Mode
Relay 4 Mode
SNMP Destination IP(s)
SMTP Server IP/DNS
Local e-mail (FROM:)
Destination e-mail(s) (TO:)

SERIAL 1 |
Baud rate |
Data bits |
Parity |
Stop bits |
Handshake |
UDP/TCP Control Port for COM1 |
SERIAL 2 |
Baud rate |
Data bits |
Parity |
Stop bits |
Handshake |
UDP/TCP Control Port for COM2 |

SECURITY SETTINGS |
Reset Function | Enabled Disabled
Factory Defaults | Enabled Disabled
Update Function | Enabled Disabled
&LSetup(3,"%s",130,D,0," Set Password | "); &LSetup(3,"%s",130,D,!0," | Old Password |
New Password | ");