Help Status screen Note: see the system status page or the application status page for further details on the actual device configuration. Site Type Displays the current configured site type. Stream Mode Displays the current configured event to start streaming to the remote destination(s). Keep-Alive Displays the current configured keep-alive strategy. Connection Status Displays the actual connection state. Incoming Stream Status Displays the actual incoming stream status (ON/OFF). Outgoing Stream Status Displays the actual outgoing stream status (ON/OFF). Audio Input Displays the selected input source. Audio Format Displays the incoming audio format, or the local audio format if no valid incoming RTP payload is detected. Input/Output Audio level Displays the input and output audio levels in dB, and as visual peak level graphic bar in dB. Relay 1 to 4 Shows the configured event for local relay switch. Remote Inputs Remote input state, lime color means active, gray mean inactive. Local Inputs Local input state, lime color means active, gray mean inactive. Local Relays Local relay state, lime color means active, gray mean inactive.