Enseo HD-1500 firmware update and setup instructions. (NOT DS-1500)

11/26/08

Firmware update:

 

1) Download and unzip the .txt file and copy it to a local drive.
2) Power the box. While its booting up press "Return" key in HyperTerminal the whole time. This should break the boot and you should go to prompt (something like calica> or HD-1500)
3) At the prompt type 'dpr'.
4) Select 'Send Text File' from the 'Transfer' menu in HyperTerminal. Select the firmware.txt file.
5) After you send the .txt file you should see progressing dots('.....').
6) After the download and flashing, it goes back to the HD-1500> prompt. Reboot the box. This process may take 2 hrs!
 

Note: DO Not remove power during Firmware Update. It will brick the Set Top Box.
 

The firmware update is now done.

Use 115200, 8N1

Box set up:

The box will still try to auto detect a TV and will not respond to IR remote commands after the firmware update.  The Auto detect must be disabled.

· After the flashing process in complete reboot and watch the unit boot up at the console.  When the unit is booted and running you will see it searching (auto detect) for different types of TV’s.  

· At that point type “x “ followed by a carriage return.  That will stop the auto detect process.  

· Unplug the console and connect the IR receiver to the serial port on the box.  Press “on” and then press either “menu” or “setup”.  

· Disable TV control in the ____________ menu.

· Set to “Forced on” in the ____________ menu.

http://ftp.enseo.com/swdl/craig.zip
 

