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Frequency

Ch-1
464.2250


Mt Toro Antenna and Duplexers

UHF 4, Telewave Dipole No Duplexer

Connected to Preselector and multicoupler.

Integra TR settings:

Power output 2 watts (ship units)

RX threshold –110dbm

ID 30 min.

9600 8N1 serial port

9.6 KHz TX deviation

Lobos, Flyer, Zephyr = transceiver

Toro_Lobos, Toro_Flyer, Toro_Monitor = RX only

