Rachel Carson Seatel 3011 System Set Up Notes

DAC Settings
1. System type 2
2. Dishscan off,  save PCU settings
3. Freq 0000,   This enables external ACG volts display
4. JP4 AGC jumper on TS1 board
5. Dish 1
MASC settings
1. Baud to 9600
2. Cal analog amp 0-5v input = 0-5v out
3. Cal meter to -64dbm from Moseley ODU = 0db

B&B modem
1. CH-00
2. ID 11
3. AD input-0 set to 0-2.5v = 0-5v
4. Default DO-0 off
5. Output level +10dbm
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