
 Mt. TORO SYSTEM “A” SEATEL & MICROWAVE (Pt LOBOS)


TAC-92
TAC 11301
SN 839
V1.78
REV: 04JUN04
WHEN SHIP IS IN PORT:

DISPAY MUST READ –

PRESS: 
“SHIP”
“SAT”
“ANT”

LAT:   37N              
SAT: 000E
AZ: 333.5±



LON:  121W      
THRS: 3000
EL: 0.0±

HDG: 312.5 
EXT RCVR
REL:  N/A


AGC: 3100+
AGC: 3100+

PROGRAMMABLE PARAMETERS

Press “MODE” to step through the following menus
CONTROL TRACKING:     
ON (SWITCHED BY THE AUX1 KEY)
SEARCHING:       
OFF
STANDBY:       
OFF

Continue Pressing “MODE” and you will enter the “STATUS” menu

STATUS

*ERROR:     
0000
AZ: 2124        EL: 2015

Continue Pressing “MODE” and you will enter the “SET-UP” menu
(ENTER 7979 TO ENTER SET-UP IF THE DISPLAY IS LOCKED)

SET-UP

AUTO CAL

EL SCALE:       
8310

EL TRIM:       
0108 (SETS EL TO Ø°±)

AZ SCALE:
4180

AZ TRIM:       
0145

STEP SIZE:**   
 001   
000  
 
STEP DELAY:         
010

STEP INTREGAL:
040

AUTO THRES:
000
SEARCH INC:    
000
SEARCH LIMIT:      
006
SEARCH DELAY:       
000

SYSTEM TYPE:        
001

GYRO TYPE:       
000
ALL POLANGS WHICH FOLLOW ARE:     000

ITEMS IN RED DENOTE ENTRIES THAT WILL RESET UPON AN AC POWER FAILURE AND ARE IMPORTANT.

(IF THE HIGHLIGHTED READINGS ARE NOT AS SHOWN ABOVE, PRESS THE APRPOPRIATE BUTTON TO STEP TO THE INCORRECT ENTRY AND ENTER THE CORRECT VALUE.)

* PLEASE NOTE ANY ERRORS. TO CLEAR ERRORS, PRESS  THE “” KEY.

** VALUES MUST BE SET VIA THE SERIAL PORT
MICROWAVE

RECEIVER
CH 14  (6512.5MHz)

TRANSMITTER
CH 2   (6462.5MHz)


 Mt. TORO SYSTEM “B” SEATEL & MICROWAVE (WESTERN FLYER)


TAC-92
RAC 10001
SN 595
V1.80
REV: 04JUN04
WHEN SHIP IS IN PORT:

DISPAY MUST READ –

PRESS: 
“SHIP”
“SAT”
“ANT”

LAT:   37N              
SAT: 000E
AZ : 333.5±



LON:  121W      
THRS: 3000
EL: 0.0±

HDG: 312.5 
EXT RCVR
REL:  N/A


AGC: 3000+
AGC: 3000+


PROGRAMMABLE PARAMETERS

Press “MODE” to step through the following menus
CONTROL TRACKING:     
ON (SWITCHED BY THE AUX1 KEY)
SEARCHING:       
OFF
STANDBY:       
OFF

Continue Pressing “MODE” and you will enter the “STATUS” menu

STATUS

*ERROR:     
0000
AZ: 2624        EL: 2004
Continue Pressing “MODE” and you will enter the “SET-UP” menu
(ENTER 7979 TO ENTER SET-UP IF THE DISPLAY IS LOCKED)
SET-UP

AUTO CAL

EL SCALE:       
9300

EL TRIM:       
0095 (SETS EL TO Ø°±)

AZ SCALE:
4200

AZ TRIM:       
0100
STEP SIZE:**    
 001   
000  
 
STEP DELAY:         
010

STEP INTREGAL:
040

AUTO THRES:
000
SEARCH INC:    
000
SEARCH LIMIT:      
006
SEARCH DELAY:       
000

SYSTEM TYPE:        
001

GYRO TYPE:       
000
ALL POLANGS WHICH FOLLOW ARE:     000

ITEMS IN RED DENOTE ENTRIES THAT WILL RESET UPON AN AC POWER FAILURE AND ARE IMPORTANT.

(IF THE HIGHLIGHTED READINGS ARE NOT AS SHOWN ABOVE, PRESS THE APRPOPRIATE BUTTON TO STEP TO THE INCORRECT ENTRY AND ENTER THE CORRECT VALUE.)

* PLEASE NOTE ANY ERRORS. TO CLEAR ERRORS, PRESS  THE “” KEY.

** VALUES MUST BE SET VIA THE SERIAL PORT

MICROWAVE

RECEIVER
CH 11  (6437.5MHz)

TRANSMITTER
CH 13 (6487.5MHz) NEW STYLE MRC XMTR
