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WHEN SHIP IS IN PORT:

DISPAY MUST READ –

PRESS: 
“SHIP”
“SAT”
“ANT”

LAT:  36N              
SAT:  000E
AZ:   153.0±



LON: 122W      
THRS: 2700
EL:  0.0±

HDG:  204.0± 
EXT RCVR
REL:  N/A

204
AGC:  3100+
AGC:  3100+

PROGRAMMABLE PARAMETERS

Press “MODE” to step through the following menus
CONTROL TRACKING:     
ON
CONTROL SEARCH 1:       
OFF
CONTROL SEARCH 2:       
OFF

Continue Pressing “MODE” and you will enter the “STATUS” menu
STATUS

*ERROR:     
0000
REMOTE AUX:
5535

Continue Pressing “MODE” and you will enter the “SET-UP” menu
(Press “7979“ to enter SET-UP if the display is locked)
SET-UP

EL TRIM:       
0000

AZ TRIM:       
-0030

AGC THRESHOLD:   
0000  
 
EL STEP SIZE:       
0000
AZ STEP SIZE:       
0003

STEP DELAY:         
0002
SEARCH INC:    
0006
SEARCH LIMIT:      
0200
SEARCH DELAY:       
0005

STEP INTREGAL
0080

SYSTEM TYPE:        
0026

GYRO TYPE:       
0002 (confirm)
ALL POLANGS WHICH FOLLOW ARE:     000

* PLEASE NOTE ANY ERRORS. TO CLEAR ERRORS, PRESS  THE “” KEY.

ITEMS IN RED DENOTE ENTRIES THAT WILL RESET UPON AN AC POWER FAILURE AND ARE IMPORTANT.

(IF THE HIGHLIGHTED READINGS ARE NOT AS SHOWN ABOVE, PRESS THE APRPOPRIATE BUTTON TO STEP TO THE INCORRECT ENTRY AND ENTER THE CORRECT VALUE.)
MICROWAVE EQUIPMENT IN THE VOID
INSURE THE EQUIPMENT IS TURNED ON AND THE CHANNELS ARE SET AS FOLLOWS:
RECEIVER
CH13 (6487.5 MHz)

TRANSMITTER
CH 1  (6437.5 MHz)
