
TESTING A 6 GHz TRANSMITTER


POWER ON


A-YES
B-NO

TURN POWER ON


C-FILTER SWITCH CORRECT
GO BACK TO (A)


(IF APPLICABLE)


D-NO
E-YES

SWITCH FILTER(S)
PERFORM SYSTEM  SELFCHECK


GO TO (E)
(SWITCH RECEIVER TO TRANSMIT


FREQUENCY AND NOTE SIGNAL 


STRENGTH)

 
F-SIGNAL STRENGTH 
G-SIGNAL STRENGTH


ACCEPTABLE
NOT ACCEPTABLE


TRANSMITTER OK
TRANSMITTER BAD


CHECK VIDEO QUALITY
REMOVE FROM SERVICE.


INSTALL SPARE


GO BACK TO (E)

