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VIDEO 
AUDIO

IN
L
R
1 -
MBARI A - 6 GHz (PL) RCVR VIDEO OUT
UHF RCVR
RCVR AUDIO CH 1

2 -
MBARI B - 18 GHz (PL) RCVR VIDEO OUT
RCVR AUDIO CH 2
RCVR AUDIO CH 1


3 -
MBARI B - 18 GHz (MBA) RCVR VIDEO OUT
RCVR AUDIO CH 2
RCVR AUDIO CH 1

4 - MBARI B - 6 GHz (WF) RCVR VIDEO OUT
RCVR AUDIO CH 2
RCVR AUDIO CH 1

5 -
MBARI C - 18 GHz (WF) RCVR VIDEO OUT
RCVR AUDIO CH 3
RCVR AUDIO CH 2

6 -
N/C
N/C
N/C

7 -
TORO CAM
N/C
N/C

8 - MAGNI WFG (BARS)
+4 dBm TONE
+4 dBm TONE


VIDEO
AUDIO

OUT
L
R
1 -
MBARI A - 6 GHz (PL) XMTR VIDEO IN
XMTR AUDIO CH 2
XMTR AUDIO CH 1

2 -
MBARI A - 18 GHz (PL) XMTR VIDEO IN
XMTR AUDIO CH 2
XMTR AUDIO CH 1

3 -
MBARI C - 18 GHz (MBA) XMTR VIDEO IN
XMTR AUDIO CH 2
XMTR AUDIO CH 1 

4 - MBARI B - 6 GHz (WF) XMTR VIDEO IN
XMTR AUDIO CH 2
XMTR AUDIO CH 1 

5 - MBARI C - 18 GHz (WF) XMTR VIDEO IN
XMTR AUDIO CH 3
XMTR AUDIO CH 2

6 -
N/C
N/C
N/C


7 -
VIDEO MONITOR 2
N/C
VIDEO MONITOR 2



8 -
VIDEO MONITOR 1
VIDEO MONITOR 1
N/C

STORED AS PATTERN 1 (DEFAULT), SEE REVERSE SIDE
TO RECALL PATTERN 1: PRESS “R”, “1”, “EN”
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*UHF RCVR AUDIO

