Script started on Tue ar 24 10:35:34 1998


orca:/users/teto[31]> cd /users/teto/kermit


orca:/users/teto/kermit[32]> wermit


C-Kermit 6.0.192, 6 Sep 96, for HP-UX 9.0


 Copyright (C) 1985, 1996,


  Trustees of Columbia University in the City of New York.


Default file-transfer mode is TEXT


Type ? or HELP for help.


[/users/teto/kermit] C-Kermit>set l /dev/cua00


[/users/teto/kermit] C-Kermit>set sp 19200


/dev/cua00, 19200 bps


[/users/teto/kermit] C-Kermit>c


Connecting to /dev/cua00, speed 19200.


The escape character is Ctrl-\ (ASCII 28, FS)


Type the escape character followed by C to get back,


or followed by ? to see other options.


ate1q0v1                < Won't echo have to type in blind.  


at&n2                   < Forces maximum speed to be 1200


OK


atdt9,6022058


CONNECT 1200/ARQ/LAP/V42BIS








Lantronix ETS16 Version B3.3/304(950119)





Type HELP at the 'Local_16> ' prompt for assistance.





Username> teto          < Doesn't matter.





Local_16> connect @@seatel


Connecting session 1 to service  at node PL_LANTRONIX  port SEATEL 


Lat protocol emulation V5.2 





Send a break to get back to the terminal server.





